|  |  |
| --- | --- |
| **TABLE 5**  **OAR 340-200-0020(60)**  **GENERIC PSELS** | |
| **Pollutant** | **Generic PSEL (tons/year, except as noted)** |
| GreenhouseGases (CO2e) | 74,000 |
| CO | 99 |
| NOx | 39 |
| SO2 | 39 |
| VOC | 39 |
| PM | 24 |
| PM10 (except Medford AQMA) | 14 |
| PM10/PM2.5 (Medford AQMA) | 4.5 [49 lbs/day] |
| Direct PM2.5 | 9 |
| Lead | 0.5 |
| Fluorides | 2 |
| Sulfuric Acid Mist | 6 |
| Hydrogen Sulfide | 9 |
| Total Reduced Sulfur (including hydrogen sulfide) | 9 |
| Reduced Sulfur | 9 |
| Municipal waste combustor organics (Dioxin and furans) | 0.0000030 |
| Municipal waste combustor metals | 14 |
| Municipal waste combustor acid gases | 39 |
| Municipal solid waste landfill gases | 49 |
| Single HAP | 9 |
| Combined HAPs (aggregate) | 24 |