|  |
| --- |
| **TABLE 4****OAR 340-200-0020(33)****DE MINIMIS EMISSION LEVELS** |
| **Pollutant** | **De minimis (tons/year, except as noted)** |
| Greenhouse Gases (CO2e) | 2,756 |
| CO | 1 |
| NOx | 1 |
| SO2 | 1 |
| VOC | 1 |
| PM | 1 |
| PM10 (except Medford AQMA) | 1 |
| PM10/PM2.5 (Medford AQMA) | 0.5 [5.0 lbs/day] |
| Direct PM2.5  | 1 |
| Lead  | 0.1 |
| Fluorides | 0.3 |
| Sulfuric Acid Mist | 0.7 |
| Hydrogen Sulfide | 1 |
| Total Reduced Sulfur (including hydrogen sulfide) | 1 |
| Reduced Sulfur | 1 |
| Municipal waste combustor organics (Dioxin and furans) | 0.0000005 |
| Municipal waste combustor metals | 1 |
| Municipal waste combustor acid gases | 1 |
| Municipal solid waste landfill gases | 1 |
| Single HAP  | 1 |
| Combined HAP (aggregate) | 1 |