**340-234-0510**

|  |
| --- |
| **Veneer and Plywood Manufacturing Operations**(1) Veneer Dryers: (b) No person shall operate any veneer dryer such that visible air contaminants emitted from any dryer stack or emission point exceed:  |
| Existing Rule language | Option 1 | Option 2 | Option 3 |
| (A) An average operating opacity of ten percent; and (B) A maximum opacity of 20 percent."Average Operating Opacity" means the opacity of emissions determined using EPA Method 9 on any three days within a 12-month period which are separated from each other by at least 30 days; a violation of the average operating opacity limitation is judged to have occurred if the opacity of emissions on each of the three days is greater than the specified average operating opacity limitation."Maximum Opacity" means the opacity as determined by EPA Method 9 (average of 24 consecutive observations). | (A) A daily average operating opacity of 10 percent on more than two days within any 12-month period, with the days separated from each other by at least 30 days, and with opacity determined by EPA Method 9; or (B) A maximum opacity of 20 percent as measured by EPA Method 9 at any time. | (A) A daily average operating opacity of 10 percent on more than two days within any 12-month period that are separated from each other by at least 30 days, as determined by EPA Method 9; or (B) A maximum opacity of 20 percent at any time as measured by EPA Method 9. | (A) An average operating opacity of 10 percent on at least three days within any 12-month period which are separated from each other by at least 30 days, as determined using EPA Method 9; or (B) A maximum opacity of 20 percent at any time, as measured using EPA Method 9. |