|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Source** | **Permit No.** | **Location** | **PM2.5 Monitoring (’10-’12)** | **Emissions Unit** | **Source Test Results** | **Comment** |
| Boise Cascade | 30-0016 | Pilot Rock | ~22 µg/m3 (Pendleton) | 3 wood-fired boilers | **0.06**-**0.19** | Backup to natural gas fired boiler. |
| Collins Sawmill | 19-0002 | Fremont | 33 µg/m3  (Lakeview) | 2 wood-fired boilers | **0.08 - 0.13** |  |
| Columbia Forest Products | 18-0014 | Klamath Falls | 35 µg/m3 | 2 wood-fired boilers | **0.08** – **0.19** |  |
| Interfor Pacific | 18-0005 | Gilchrist | ~18 µg/m3  (Bend) | 2 wood-fired boilers | **0.086** - **0.21** |  |
| Frank Lumber | 22-2525 | Lyons | ~22 µg/m3  (Sweet Home) | Wood fired boiler | **0.137** | multiclone |
| Swanson Group | 10-0030 | Roseburg | ~27 µg/m3 | Wood fired boiler | **0.17** | HF < 26,800 lb/hr steam  NG > 26,800 lb/hr steam |
| Harney Rock and Paving | 13-0010 | Burns | 30 µg/m3 | **Asphalt plant** | **0.22** | (1992 ST) |
| Rogers Asphalt Paving | 31-0001 | Island City | ~20 µg/m3  (La Grande) | **Asphalt plant** | **0.11** |  |