**DIVISION 200**

**GENERAL AIR POLLUTION PROCEDURES AND DEFINITIONS**

**340-200-8005**

**Table 1 Significant Impact Levels**

As used in divisions 200, 209, and 225, Table 1 Significant Impact Levels refers to the table below.

| Table 1  **Significant Impact Levels** | | | | | |
| --- | --- | --- | --- | --- | --- |
| Pollutant | Averaging Time | Air Quality Area Designation | | | |
| Class I | Class II | Class III | |
| SO2 (µg/m3)[[1]](#footnote-1) | Annual | 0.10 | 1.0 | 1.0 |  |
| 24-hour | 0.20 | 5.9 | 5.0 |  |
| 3-hour | 1.0 | 25.0 | 25.0 |  |
| PM10 (µg/m3) | Annual | 0.20 | 0.20 | 0.20 |  |
| 24-hour | 0.30 | 1.0 | 1.0 |  |
| PM2.5 (µg/m3) | Annual | 0.06 | 0.3 | 0.3 |  |
| 24-hour | 0.07 | 1.2 | 1.2 |  |
| NO2 (µg/m3) | Annual | 0.10 | 1.0 | 1.0 |  |
| CO (mg/m3)[[2]](#footnote-2) | 8-hour | --- | 0.5 | 0.5 |  |
| 1-hour | --- | 2.0 | 2.0 |  |

     [ED. NOTE: This rule amended and renumbered from OAR 340-200-0020.]

|  | | |
| --- | --- | --- |
|  |  | |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  | |

|  | | | |
| --- | --- | --- | --- |
|  |  | | |
|  |  |  |  |
|  |  |  | |

|  | | |
| --- | --- | --- |
|  |  | |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  | |
|  |  | |
|  |  | |

|  | | |
| --- | --- | --- |
|  |  | |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  | |
|  |  | |
|  |  | |
|  |  | |

1. Micrograms/cubic meter [↑](#footnote-ref-1)
2. Millligrams/cubic meter [↑](#footnote-ref-2)