| Table # 1  **PSD Increments (Maximum Allowable Increase)**  **(micrograms per cubic meter)**  **OAR 340-202-8000** | | |
| --- | --- | --- |
| **Class I** | | |
| Pollutant | Increment |  |
| Particulate Matter: |  |  |
| PM2.5, annual arithmetic mean | 1 |  |
| PM2.5, 24-hour maximum | 2 |  |
| PM10, annual arithmetic mean | 4 |  |
| PM10, 24-hour maximum | 8 |  |
| Sulfur dioxide: |  |  |
| annual arithmetic mean | 2 |  |
| 24-hour maximum | 5 |  |
| 3-hour maximum | 25 |  |
| Nitrogen dioxide: |  |  |
| annual arithmetic mean | 2.5 |  |
| **Class II** | | |
| Pollutant | Increment | |
| Particulate Matter: |  | |
| PM2.5, annual arithmetic mean | 4 | |
| PM2.5, 24-hour maximum | 9 | |
| PM10, annual arithmetic mean | 17 | |
| PM10, 24-hour maximum | 30 | |
| Sulfur dioxide: |  | |
| annual arithmetic mean | 20 | |
| 24-hour maximum | 91 | |
| 3-hour maximum | 512 | |
| Nitrogen dioxide: |  | |
| annual arithmetic mean | 25 | |
| **Class III** | | |
| Pollutant | Increment | |
| Particulate Matter: |  | |
| PM2.5, annual arithmetic mean | 8 | |
| PM2.5, 24-hour maximum | 18 | |
| PM10, annual arithmetic mean | 34 | |
| PM10, 24-hour maximum | 60 | |
| Sulfur dioxide: |  | |
| annual arithmetic mean | 40 | |
| 24-hour maximum | 182 | |
| 3-hour maximum | 700 | |
| Nitrogen dioxide: |  | |
| annual arithmetic mean | 50 | |