| Table # 1**PSD Increments (Maximum Allowable Increase)****(micrograms per cubic meter)****OAR 340-202-8000** |
| --- |
| **Class I** |
| Pollutant | Increment |  |
| Particulate Matter: |  |  |
| PM2.5, annual arithmetic mean | 1 |  |
| PM2.5, 24-hour maximum | 2 |  |
| PM10, annual arithmetic mean | 4 |  |
| PM10, 24-hour maximum | 8 |  |
| Sulfur dioxide: |  |  |
| annual arithmetic mean | 2 |  |
| 24-hour maximum | 5 |  |
| 3-hour maximum | 25 |  |
| Nitrogen dioxide: |  |  |
| annual arithmetic mean | 2.5 |  |
| **Class II** |
| Pollutant | Increment |
| Particulate Matter: |  |
| PM2.5, annual arithmetic mean | 4 |
| PM2.5, 24-hour maximum | 9 |
| PM10, annual arithmetic mean | 17 |
| PM10, 24-hour maximum | 30 |
| Sulfur dioxide: |  |
| annual arithmetic mean | 20 |
| 24-hour maximum | 91 |
| 3-hour maximum | 512 |
| Nitrogen dioxide: |  |
| annual arithmetic mean | 25 |
| **Class III** |
| Pollutant | Increment |
| Particulate Matter: |  |
| PM2.5, annual arithmetic mean | 8 |
| PM2.5, 24-hour maximum | 18 |
| PM10, annual arithmetic mean | 34 |
| PM10, 24-hour maximum | 60 |
| Sulfur dioxide: |  |
| annual arithmetic mean | 40 |
| 24-hour maximum | 182 |
| 3-hour maximum | 700 |
| Nitrogen dioxide: |  |
| annual arithmetic mean | 50 |