“modified source”

(55) “Federal Major Source” means a source with potential to emit any individual regulated pollutant, excluding hazardous air pollutants listed in OAR 340 division 244, greater than or equal to 100 tons per year if in a source category listed below, or 250 tons per year if not in a source category listed. In addition, for greenhouse gases, a federal major source must also have the potential to emit CO2e greater than or equal to 100,000 tons per year. The fugitive emissions and insignificant activity emissions of a stationary source are considered in determining whether it is a federal major source. Potential to emit calculations must include emission increases due to a new or modified source and may include emission decreases.

(68) "Lowest Achievable Emission Rate" or "LAER" means that rate of emissions which reflects: the most stringent emission limitation which is contained in the implementation plan of any state for such class or category of source, unless the owner or operator of the proposed source demonstrates that such limitations are not achievable; or the most stringent emission limitation which is achieved in practice by such class or category of source, whichever is more stringent. The application of this term cannot permit a proposed new or modified source to emit any air contaminant in excess of the amount allowable under applicable New Source Performance Standards (NSPS) or standards for hazardous air pollutants.

(72) "Major Source":

(a) Except as provided in subsection (b) of this section, means a source that emits, or has the potential to emit, any regulated air pollutant at a Significant Emission Rate. The fugitive emissions and insignificant activity emissions of a stationary source are considered in determining whether it is a major source. Potential to emit calculations must include emission increases due to a new or modified source and may include emission decreases.

“Netting Basis”

(d) Netting basis is zero for:

(A) Any regulated pollutant emitted from a source that first obtained permits to construct and operate after the applicable baseline period for that regulated pollutant, and has not undergone New Source Review for that pollutant;

(B) Any pollutant that has a generic PSEL in a permit;

(C) Any source permitted as portable; or

(D) Any source with a netting basis calculation resulting in a negative number.

(e) If a source relocates to an adjacent site, and the time between operation at the old and new sites is less than six months, the source may retain the netting basis from the old site.

(f) Emission reductions required by rule, order, or permit condition affect the netting basis if the source currently has devices or emissions units that are subject to the rules, order, or permit condition. The baseline emission rate is not affected. The netting basis reduction will be effective on the effective date of the rule, order, or permit condition requiring the reduction. The PSEL reduction will be effective on the compliance date of the rule, order, or permit condition.

(g) For permits issued after May 1, 2011 under New Source Review regulations in OAR 340 division 224, and where the netting basis initially equaled the potential to emit for a new or modified source, the netting basis will be reduced in accordance with the definition of actual emissions. Notwithstanding OAR 340-222-0041(2), this adjustment does not require a reduction in the PSEL.

(146) "Typically Achievable Control Technology" or "TACT" means the emission limit established on a case-by-case basis for a criteria pollutant from a particular emissions unit in accordance with OAR 340-226-0130. For existing sources, the emission limit established will be typical of the emission level achieved by emissions units similar in type and size. For new and modified sources, the emission limit established will be typical of the emission level achieved by well controlled new or modified emissions units similar in type and size that were recently installed. TACT determinations will be based on information known to the Department while considering pollution prevention, impacts on other environmental media, energy impacts, capital and operating costs, cost effectiveness, and the age and remaining economic life of existing emission control equipment. The Department may consider emission control technologies typically applied to other types of emissions units where such technologies could be readily applied to the emissions unit. If an emission limitation is not feasible, a design, equipment, work practice, operational standard, or combination thereof, may be required.

### 340-202-0210

### Ambient Air Increments

(1) This rule defines significant deterioration. In areas designated as Class I, II or III, emissions from new or modified sources must be limited such that increases in pollutant concentration over the baseline concentration must be limited to those set out in Table 1.

### 340-210-0230

### Notice to Construct

(1) Any person proposing a Type 1 or 2 change must provide notice to the Department before constructing or modifying a stationary source or air pollution control equipment. The notice must be in writing on a form supplied by the Department and include the following information as applicable:

(a) Name, address, and nature of business;

(b) Name of local person responsible for compliance with these rules;

(c) Name of person authorized to receive requests for data and information;

(d) The type of construction or modification as defined in OAR 340-210-0220;

(e) A description of the constructed or modified source;

(f) A description of the production processes and a related flow chart for the constructed or modified source;

(g) A plot plan showing the location and height of the constructed or modified source. The plot plan must also indicate the nearest residential or commercial property;

(10) "Ozone Precursor Distance" means the distance in kilometers from the nearest boundary of a designated ozone nonattainment or maintenance area within which a major new or modified source of VOC or NOx is considered to significantly affect that designated area. The determination of significance is made by either the formula method or the demonstration method.

(11) "Ozone Precursor Offsets" means the emission reductions required to offset emission increases from a major new or modified source located inside the designated nonattainment or maintenance area or within the Ozone Precursor Distance. Emission reductions must come from within the designated area or from within the Ozone Precursor Distance of the offsetting source as described in OAR 340-225-0090. The offsets determination is made by either the formula method or the demonstration method.

(a) The Formula Method.

(A) Required offsets (RO) for new or modified sources are determined as follows:

### 340-225-0090

### Requirements for Demonstrating a Net Air Quality Benefit

Demonstrations of net air quality benefit for offsets must include the following:

(1) Ozone areas (VOC and NOx emissions). For sources capable of impacting a designated ozone nonattainment or maintenance area;

(a) Offsets for VOC and NOx are required if the source will be located within the designated area or within the Ozone Precursor Distance.

(b) The amount and location of offsets must be determined in accordance with this subsection:

(A)For new or modified sources locating within a designated nonattainment area, the offset ratio is 1.1:1. These offsets must come from within either the same designated nonattainment area as the new or modified source or another ozone nonattainment area (with equal or higher nonattainment classification) that contributes to a violation of the NAAQS in the same designated nonattainment area as the new or modified source.

(B) For new or modified sources locating within a designated maintenance area, the offset ratio is 1.1:1. These offsets may come from within either the designated area or the ozone precursor distance.

(C) For new or modified sources locating outside the designated area, but within the ozone precursor distance, the offset ratio is 1:1. These offsets may come from within either the designated area or the ozone precursor distance

1. Medford-Ashland AQMA: Proposed new major PM10 sources or major PM10 modifications locating within the AQMA that are required to provide emission offsets under OAR 340-224-0060(2)(a) must provide reductions in PM10 emissions equal to 1.2 times the emissions increase over the netting basis from the new or modified source, and must provide a net air quality benefit within the AQMA. "Net Air Quality Benefit" means:

### 340-226-0130

### Typically Achievable Control Technology (TACT)

(1) Existing Sources. An existing emissions unit must meet TACT for existing sources if:

(a) The emissions unit is not already subject to emission standards under OAR 340-232-0010 through 340-232-0240, OAR 340 Divisions 230, 234, 236, or 238, OAR 340-240-0110 through 340-240-0180, 340-240-0310(1), OAR 340-240-0320 through 340-240-0430, or OAR 340 Division 224 for the pollutant emitted;

(b) The source is required to have a permit;

(c) The emissions unit has emissions of criteria pollutants equal to or greater than 5 tons per year of particulate or 10 tons per year of any gaseous pollutant; and

(d) The Department determines that air pollution control equipment and emission reduction processes in use for the emissions unit do not represent TACT, and that further emission control is necessary to address documented nuisance conditions, address an increase in emissions, ensure that the source is in compliance with other applicable requirements, or protect public health or welfare or the environment.

(2) New and Modified Sources. A new or modified emissions unit must meet TACT for new or modified sources if:

(a) The new or modified emissions unit is not subject to New Source Review requirements in OAR 340 division 224, an applicable Standard of Performance for New Stationary Sources in OAR 340 division 238, OAR 340-240-0110 through 340-240-0180, 340-240-0310(1), OAR 340-240-320 through 340-240-0430, or any other standard applicable only to new or modified sources in OAR 340 divisions 230, 234, 236, or 238 for the pollutant emitted;

**340-234-0210 (Pulp Mill Rules)**

**Emission Limitations**

(5) New Source Performance Standards. New or modified sources that commenced construction after September 24, 1976, are subject to each provision of this rule and the New Source Performance Standards, 40 CFR 60 subpart BB as adopted under OAR 340-238-0060, whichever is more stringent.

**340-240-0030**

(25) "Modified Source" means any source with a major modification as defined in OAR 340-200-0020.

(36) "Rebuilt Boiler" means a physical change after April 29, 1988, to a wood-waste boiler or its air-contaminant emission control system which is not considered a "modified source" and for which the fixed, depreciable capital cost of added or replacement components equals or exceeds fifty percent of the fixed depreciable cost of a new component which has the same productive capacity.