**DEPARTMENT OF ENVIRONMENTAL QUALITY**

**DIVISION 240**

**RULES FOR AREAS WITH UNIQUE
AIR QUALITY NEEDS**

**340-240-0010**

**Purpose**

The purpose of this division is to address the air quality control needs of the Medford-Ashland AQMA and Grants Pass UGB (OAR 340-240-0100 through 340-240-0270), the La Grande UGB (340-240-0300 through 340-240-0360, the Lakeview UGB ( 340-240-0400 through 340-240-0440), and the Klamath Falls Nonattainment Area (340-240-0500 through 340-240-0630).

[NOTE: These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 22-1989, f. & cert. ef. 9-26-89; DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0005

**340-240-0020**

**Emission Limitations**

Emission limitations established herein and stated in terms of pounds per 1,000 square feet of production are to be computed on an hourly basis using the maximum 8 hour production capacity of the plant.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468.020 & ORS 468A.025
Hist.: DEQ 3-1996, f. & cert. ef. 1-29-96; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0007; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**340-240-0030**

**Definitions**

The definitions in OAR 340-200-0020, 340-204-0010 and this rule apply to this division. If the same term is defined in this rule and 340-200-0020 or 340-204-0010, the definition in this rule applies to this division.

(1) "Air contaminant" means a dust, fume, gas, mist, odor, smoke, vapor, pollen, soot, carbon, acid or particulate matter, or any combination thereof.

(2) "Air Conveying System" means an air moving device, such as a fan or blower, associated ductwork, and a cyclone or other collection device, the purpose of which is to move material from one point to another by entrainment in a moving airstream.

(3) "Average Operating Opacity" means the opacity of emissions determined using EPA Method 9 on any three days within a 12-month period which are separated from each other by at least 30 days; a violation of the average operating opacity limitation is judged to have occurred if the opacity of emissions on each of the three days is greater than the specified average operating opacity limitation.

(4) “Certified” includes catalytic and non-catalytic designs, unless otherwise specified.

(5) "Charcoal Producing Plant" means an industrial operation which uses the destructive distillation of wood to obtain the fixed carbon in the wood.

(6) "Collection Efficiency" means the overall performance of the air cleaning device in terms of ratio of weight of material collected to total weight of input to the collector.

(7) "Department" means Department of Environmental Quality.

(8) "Design Criteria" means the numerical as well as verbal description of the basis of design, including but not necessarily limited to design flow rates, temperatures, humidities, contaminant descriptions in terms of types and chemical species, mass emission rates, concentrations, and specification of desired results in terms of final emission rates and concentrations, and scopes of vendor supplies and owner-supplied equipment and utilities, and a description of any operational controls.

(9) "Domestic Waste" means combustible household waste, other than wet garbage, such as paper, cardboard, leaves, yard clippings, wood, or similar materials generated in a dwelling housing four (4) families or less, or on the real property on which the dwelling is situated.

(10) "Dry Standard Cubic Foot" means the amount of gas that would occupy a volume of one cubic foot, if the gas were free of uncombined water at standard conditions.

(11) "Emission" means a release into the outdoor atmosphere of air contaminants.

(12) "EPA Method 9" means the method for Visual Determination of the Opacity of Emissions From Stationary Sources described as Method (average of 24 consecutive observations) in the Department Source Sampling Manual (January, 1992).

(13) "Facility" means an identifiable piece of process equipment. A stationary source may be comprised of one or more pollutant-emitting facilities.

(14) “Fireplace” is defined in OAR 340-262-0450

(15) "Fuel Burning Equipment" means a device that burns a solid, liquid, or gaseous fuel, the principal purpose of which is to produce heat or power by indirect heat transfer. All stationary gas turbines are considered Fuel Burning Equipment. Marine installations and internal combustion engines are not considered Fuel Burning Equipment.

(16) "Fuel Moisture Content By Weight Greater Than 20 Percent" means bark, hogged wood waste, or other wood with an average moisture content of more than 20 percent by weight on a wet basis as used for fuel in the normal operation of a wood-fired veneer dryer as measured by ASTM D4442-84 during compliance source testing.

(17) "Fuel Moisture Content By Weight Less Than 20 Percent" means pulverized ply trim, sanderdust, or other wood with an average moisture content of 20 percent or less by weight on a wet basis as used for fuel in the normal operation of a wood-fired veneer dryer as measured by ASTM D4442-84 during compliance source testing.

(18) "Fugitive Emissions" means dust, fumes, gases, mist, odorous matter, vapors, or any combination thereof not easily given to measurement, collection and treatment by conventional pollution control methods.

(19) "Grants Pass Urban Growth Area" and "Grants Pass Area" means the area within the Grants Pass Urban Growth Boundary as shown on the Plan and Zoning Maps for the City of Grants Pass as of 1 February 1988.

(20) "Hardboard" means a flat panel made from wood that has been reduced to basic wood fibers and bonded by adhesive properties under pressure.

(21) “Klamath Falls Nonattainment Area” means the area as defined in OAR 340-204-0010.

(22) "La Grande Urban Growth Area" means the area within the La Grande Urban Growth Boundary as shown on the Plan and Zoning Maps for the City of La Grande as of 1 October 1991.

(23) "Lakeview Urban Growth Area" means the area within the Lakeview Urban Growth Boundary as shown on the Plan and Zoning Maps for the Town of Lakeview as of 25 October 1993.

(24) "Liquefied petroleum gas" has the meaning given by the American Society for Testing and Materials in ASTM D1835-82, "Standard Specification for Liquid Petroleum Gases."

(25) "Lowest Achievable Emission Rate" or "LAER" is defined in OAR 340-200-0020.

(26) "Maximum Opacity" means the opacity as determined by EPA Method 9 (average of 24 consecutive observations).

(27) "Medford-Ashland Air Quality Maintenance Area" (AQMA) means the area defined as beginning at a point approximately two and quarter miles northeast of the town of Eagle Point, Jackson County, Oregon at the northeast corner of Section 36, Township 35 South, Range 1 West (T35S, R1W); thence South along the Willamette Meridian to the southeast corner of Section 25, T37S, R1W; thence southeast along a line to the southeast corner of Section 9, T39S, R2E; thence south-southeast along line to the southeast corner of Section 22, T39S, R2E; thence South to the southeast corner of Section 27, T39S, R2E; thence southwest along a line to the southeast corner of Section 33, T39S, R2E; thence West to the southwest corner of Section 31, T39S, R2E; thence northwest along a line to the northwest corner of Section 36, T39S, R1E; thence West to the southwest corner of Section 26, T39S, R1E; thence northwest along a line to the southeast corner of Section 7, T39S, R1E; thence West to the southwest corner of Section 12, T39S, R1W, T39S, R1W; thence northwest along a line to southwest corner of Section 20, T38S, R1W; thence West to the southwest corner of Section 24, T38S, R2W; thence northwest along a line to the southwest corner of Section 4, T38S, R2W; thence West to the southwest corner of Section 6, T38S, R2W; thence northwest along a line to the southwest corner of Section 31, T37S, R2W; thence North and East along the Rogue River to the north boundary of Section 32, T35S, R1W; thence East along a line to the point of beginning.

(28) "Modified Source" means any source with a major modification as defined in OAR 340-200-0020.

(29) "Natural gas" means a naturally occurring mixture of hydrocarbon and nonhydrocarbon gases found in geologic formations beneath the earth's surface, of which the principal component is methane.

(30) "New Source" means any source not in existence prior to April 7, 1978 or any source not having a Permit as of April 7, 1978.

(31) "Odor" means that property of an air contaminant that affects the sense of smell.

(32) "Offset" is defined in OAR 340-200-0020.

(33) "Opacity" means the degree to which an emission reduces transmission of light and obscures the view of an object in the background as measured in accordance with the Department's Source Sampling Manual (January, 1992). Unless otherwise specified by rule, opacity must be measured in accordance with EPA Method 9. For all standards, the minimum observation period must be six minutes, though longer periods may be required by a specific rule or permit condition. Aggregate times (e.g. 3 minutes in any one hour) consist of the total duration of all readings during the observation period that exceed the opacity percentage in the standard, whether or not the readings are consecutive. Alternatives to EPA Method 9, such as a continuous opacity monitoring system (COMS), alternate Method 1 (LIDAR), or EPA Methods 22, or 203, may be used if approved in advance by the Department, in accordance with the Source Sampling Manual.

(34) "Open Burning" means burning conducted in such a manner that combustion air and combustion products may not be effectively controlled including, but not limited to, burning conducted in open outdoor fires, burn barrels, and backyard incinerators.

(35) "Particleboard" means matformed flat panels consisting of wood particles bonded together with synthetic resin or other suitable binders.

(36) "Particulate Matter" means all solid or liquid material, other than uncombined water, emitted to the ambient air as measured in accordance with the Department Source Sampling Manual. Particulate matter emission determinations must consist of the average of three separate consecutive runs. For sources tested using DEQ Method 5 or DEQ Method 7, each run must have a minimum sampling time of one hour, a maximum sampling time of eight hours, and a minimum sampling volume of 31.8 dscf. For sources tested using DEQ Method 8, each run must have a minimum sampling time of 15 minutes and must collect a minimum particulate sample of 100 mg. Wood waste boilers and charcoal producing plants must be tested with DEQ Method 5; veneer dryers, wood particle dryers, fiber dryers and press/cooling vents must be tested with DEQ Method 7; and air conveying systems must be tested with DEQ Method 8 (January, 1992).

(37) "Person" includes individuals, corporations, associations, firms, partnerships, joint stock companies, public and municipal corporations, political subdivisions, the state and any agencies thereof, and the federal government and any agencies thereof.

(38) "Press/Cooling Vent" means any opening through which particulate and gaseous emissions from plywood, particleboard, or hardboard manufacturing are exhausted, either by natural draft or powered fan, from the building housing the process. Such openings are generally located immediately above the board press, board unloader, or board cooling area.

(39) "Rebuilt Boiler" means a physical change after April 29, 1988, to a wood-waste boiler or its air-contaminant emission control system which is not considered a "modified source" and for which the fixed, depreciable capital cost of added or replacement components equals or exceeds fifty percent of the fixed depreciable cost of a new component which has the same productive capacity

(40) "Refuse" means unwanted material.

(41) "Refuse burning equipment" means a device designed to reduce the volume of solid, liquid, or gaseous refuse by combustion.

 (42) “Wood Fuel-Fired Device” means a device or appliance designed for wood fuel combustion, including cordwood stoves, wood stoves and fireplace stove inserts, fireplaces, wood fuel-fired cook stoves, pellet stoves and combination fuel furnaces or boilers, which burn wood fuels.

(43) "Source" means any structure, building, facility, equipment, installation or operation, or combination thereof, which is located on one or more contiguous or adjacent properties and which is owned or operated by the same person, or by persons under common control.

(44) "Standard Conditions" means a temperature of 68° Fahrenheit (20° Celsius) and a pressure of 14.7 pounds per square inch absolute (1.03 Kilograms per square centimeter).

(45) "Standard cubic foot" means the amount of gas that would occupy a volume of one cubic foot, if the gas were free of uncombined water at standard conditions. When applied to combustion flue gases from fuel or refuse burning, "standard cubic foot" also implies adjustment of gas volume to that which would result at a concentration of 12% carbon dioxide or 50% excess air.

(46) "Veneer" means a single flat panel of wood not exceeding 1/4 inch in thickness formed by slicing or peeling from a log.

(47) "Veneer Dryer" means equipment in which veneer is dried.

(48) "Wood-fired Veneer Dryer" means a veneer dryer which is directly heated by the products of combustion of wood fuel in addition to or exclusive of steam or natural gas or propane combustion.

(49) "Wigwam Fired Burner" means a burner which consists of a single combustion chamber, has the general features of a truncated cone, and is used for the incineration of wastes.

(50) "Wood Waste Boiler" means equipment which uses indirect heat transfer from the products of combustion of wood waste to provide heat or power.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

[Publications: Publications referenced are available from the agency.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468.020 & 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 9-1979, f. & ef. 5-3-79; DEQ 3-1980, f. & ef. 1-28-80; DEQ 14-1981, f. & ef. 5-6-81; DEQ 22-1989, f. & cert. ef. 9-26-89; DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 10-1995, f. & cert. ef. 5-1-95; DEQ 4-1995, f. & cert. ef. 2-17-95; DEQ 10-1995, f. & cert. ef. 5-1-95; DEQ 3-1996, f. & cert. ef. 1-29-96; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0010; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**The Medford-Ashland Air Quality Maintenance
Area and the Grants Pass Urban Growth Area**

**340-240-0100**

**Applicability**

OAR 340-240-0100 through 340-240-0250 apply in the Medford-Ashland Air Quality Maintenance Area (AQMA) and the Grants Pass Urban Growth Area (Area), except that OAR 340-240-0130, 340-240-0180, and 340-240-0190 apply only in the Medford-Ashland AQMA.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0012; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0110**

**Wood Waste Boilers**

(1) No person may cause or permit the emission of particulate matter from any boiler with a heat input capacity greater than 35 million Btu/hour unless the boiler has been equipped with emission control equipment which:

(a) Limits emissions of particulate matter to LAER as defined by the Department at the time the Department approves the control device; and

(b) Limits visible emissions such that their opacity does not exceed 5% for more than an aggregate of 3 minutes in any one hour, unless the permittee demonstrates by source test that emissions can be limited to LAER at higher visible emissions, but in no case may emissions equal or exceed 10% opacity for more than an aggregate of 3 minutes in any one hour. Specific opacity limits will be included in the Permit for each affected source.

(2) For boilers existing in the Baseline Period with a heat input capacity greater than 35 million Btu/hour, boiler mass emission limits for the purpose of establishing the facility's netting basis under OAR 340-200-0020 will be based on particulate matter emissions of 0.030 grains per dry standard cubic foot, corrected to 12% CO2.

(3) Rebuilt Boilers are subject to OAR 340-240-0110(1). Boiler mass emissions for purposes of 340-222-0041 will be based on LAER at the time the Department approves the rebuilt boiler.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468.020 & 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 29-1980, f. & ef. 10-29-80; DEQ 14-1986, f. & ef. 6-20-86; DEQ 22-1989, f. & cert. ef. 9-26-89; DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 4-1995, f. & cert. ef. 2-17-95; DEQ 22-1996, f. & cert. 10-22-96; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0015; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0120**

**Veneer Dryer Emission Limitations**

(1) No person is allowed to operate any veneer dryer such that visible air contaminants emitted from any dryer stack or emission point exceed the opacity limits specified in subsections (a) and (b) of this section or such that emissions of particulate matter exceed the mass emission limits of subsections (c) through (g) of this section:

(a) An average operating opacity of five percent; and

(b) A maximum opacity of ten percent, unless the permittee demonstrates by source test that the emission limits in subsections (c) through (g) of this section can be achieved at higher visible emissions than specified in subsections (a) and (b) of this section, but in no case may emissions exceed the visible air contaminant limitations of OAR 340-234-0510(1)(b). Specific opacity limits will be included in the Permit for each affected source;

(c) 0.30 pounds per 1,000 square feet of veneer dried (3/8" basis) for direct natural gas or propane fired veneer dryers;

(d) 0.30 pounds per 1,000 square feet of veneer dried (3/8" basis) for steam heated veneer dryers;

(e) 0.40 pounds per 1,000 square feet of veneer dried (3/8" basis) for direct wood fired veneer dryers using fuel which has a moisture content by weight less than 20 percent;

(f) 0.45 pounds per 1,000 square feet of veneer dried (3/8" basis) for direct wood fired veneer dryers using fuel which has a moisture content by weight greater than 20 percent;

(g) In addition to subsections (e) and (f) of this section, 0.20 pounds per 1,000 pounds of steam generated in boilers which exhaust combustion gases to the veneer dryer.

(2) Exhaust gases from fuel-burning equipment vented to the veneer dryer are exempt from OAR 340-228-0210.

(3) No person is allowed to operate a veneer dryer unless:

(a) The owner or operator has submitted a program and time schedule for installing an emission-control system which has been approved in writing by the Department as being capable of complying with subsections (1)(a) through (g) of this rule;

(b) The veneer dryer is equipped with an emission-control system which has been approved in writing by the Department and is capable of complying with subsections (1)(a) through (g) of this rule; or

(c) The owner or operator has demonstrated and the Department has agreed in writing that the dryer is capable of being operated and is operated in continuous compliance with subsections (1)(a) through (g) of this rule.

(4) Each veneer dryer must be maintained and operated at all times such that air contaminant generating processes and all contaminant control equipment are at full efficiency and effectiveness so that the emission of air contaminants is kept at the lowest practicable levels.

(5) No person is allowed to willfully cause or permit the installation or use of any means, such as dilution, which, without resulting in a reduction in the total amount of air contaminants emitted, conceals an emission which would otherwise violate this rule.

(6) Where effective measures are not taken to minimize fugitive emissions, the Department may require that the equipment or structures in which processing, handling and storage are done, be tightly closed, modified, or operated in such a way that air contaminants are minimized, controlled, or removed before discharge to the open air.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A

Stats. Implemented: ORS 468A.025

Hist.: DEQ 22-1989, f. & cert. ef. 9-26-89; DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0021; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0130**

**Air Conveying Systems (Medford-Ashland AQMA Only)**

All air conveying systems emitting greater than ten tons per year of particulate matter to the atmosphere must, with the prior written approval of the Department, be equipped with a control system with collection efficiency of at least 98.5 percent.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 22-1989, f. & cert. ef. 9-26-89; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0025; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0140**

**Wood Particle Dryers at Particleboard Plants**

(1) No person is allowed to cause or permit the total emission of particulate matter from all wood particle dryers at a particleboard plant site to exceed 0.40 pounds per 1,000 square feet of board produced by the plant on a 3/4" basis of finished product equivalent.

(2) No person is allowed to cause or permit the visible emissions from the wood particle dryers at a particleboard plant to exceed ten percent opacity, unless the permittee demonstrates by source test that the particulate matter emission limit in section (1) of this rule can be achieved at higher visible emissions. In no case are emissions allowed to equal or exceed 20 percent opacity. Specific opacity limits will be included in the Permit for each affected source.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 14-1981, f. & ef. 5-6-81; DEQ 14-1986, f. & ef. 6-20-86; DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0030; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0150**

**Hardboard Manufacturing Plants**

(1) Emissions from Hardboard plants excluding press vents. No person is allowed to cause or permit the total emissions of particulate matter from a hardboard plant, excluding press/cooling vents, to exceed 0.25 pounds per 1,000 square feet of hardboard produced on a 1/8" basis of finished product equivalent.

(2) Emissions from Hardboard plants including press vents. No person is allowed to cause or permit the total emissions of particulate matter from a hardboard plant, including press/cooling vents, to exceed 0.55 pounds per 1,000 square feet of hardboard produced on a 1/8" basis of finished product equivalent.

(3) When calculating emissions for this rule, emissions from truck dump and storage areas, fuel burning equipment, and refuse burning equipment are not included.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468.020 & 468A.025
Hist.: DEQ 14-1981, f. & ef. 5-6-81; DEQ 14-1986, f. & ef. 6-20-86; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 4-1995, f. & cert. ef. 2-17-95; DEQ 2-1996, f. & cert. ef. 1-29-96; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0031; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0160**

**Wigwam Waste Burners**

No person owning or controlling any wigwam burner is allowed to cause or permit the operation of the wigwam burner.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 29-1980, f. & ef. 10-29-80; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0035; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**340-240-0170**

**Charcoal Producing Plants**

(1) No person is allowed to cause or permit the emission of particulate matter from charcoal producing plant sources including, but not limited to, charcoal furnaces, heat recovery boilers, and wood dryers using any portion of the charcoal furnace off-gases as a heat source, in excess of a total from all sources within the plant site of 10.0 pounds per ton of char produced (5.0 grams per Kilogram of char produced).

(2) Emissions from char storage, briquette making, boilers not using charcoal furnace off-gases, and fugitive sources are excluded in determining compliance with section (1) of this rule.

(3) Charcoal producing plants as described in section (1) of this rule are exempt from the limitations of OAR 340-226-0210 sections (1) and (2), and 340-226-0310 which concern particulate emission concentrations and process weight.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 14-1986, f. & ef. 6-20-86; DEQ 22-1989, f. & cert. ef. 9-26-89; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0040; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**340-240-0180**

**Control of Fugitive Emissions (Medford-Ashland AQMA Only)**

(1) All sawmills, all plywood mills and veneer manufacturing plants, particleboard and hardboard plants, charcoal manufacturing plants, asphalt plants, rock crushers, animal feed manufacturers, and other major industrial facilities as identified by the Department, must prepare and implement site-specific plans for the control of fugitive emissions.

(2) Fugitive emission-control plans must identify reasonable measures to prevent particulate matter from becoming airborne. Special care will be taken by the facility to avoid the migration of material onto the public road system. Such reasonable measures include, but are not limited to the following:

(a) The systematic paving of all unpaved roads and areas on which vehicular traffic occurs. Until an area is paved, subsection (2)(b) applies;

(b) Scheduled application of asphalt, oil, water, or other suitable chemicals on unpaved roads, log storage or sorting yards, materials stockpiles, and other surfaces which can create airborne dust. Dust suppressant material must not adversely affect water quality;

(c) Periodic sweeping or cleaning of paved roads and other areas as necessary to prevent migration of material onto the public road system;

(d) Full or partial enclosure of materials stockpiled in cases where application of oil, water, or chemicals are not sufficient to prevent particulate matter from becoming airborne;

(e) Installation and use of hoods, fans, and fabric filters to enclose and vent the handling of dusty materials;

(f) Adequate containment during sandblasting or other similar operations;

(g) Covering, at all times when in motion, open bodied trucks transporting materials likely to become airborne; and

(h) Procedures for the prompt removal of earth or other material from paved streets.

(3) Reasonable measures may include landscaping and using vegetation to reduce the migration of material onto public and private roadways.

(4) The facility owner or operator must supervise and control fugitive emissions and material that may become airborne caused by the activity of outside contractors delivering or removing materials at the site.

(5) The site-specific fugitive dust emissions control plan must be submitted to the Department prior to or within 60 days of permit issuance or renewal. The Department will approve or deny the plan within 30 days.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the EQC under OAR 340-200-0040.]

Stat. Auth.: ORS 468.020
Stats. Implemented: ORS 468A.025
Hist.: DEQ 6-1983, f. & ef. 4-18-83; DEQ 22-1989, f. & cert. ef. 9-26-89; DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 4-1995, f. & cert. ef. 2-17-95; DEQ 10-1995, f. & cert. ef. 5-1-95; DEQ16-1998, f. & cert. ef. 9-23-98; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0043; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0190**

**Requirement for Operation and Maintenance Plans (Medford-Ashland AQMA Only)**

(1) Operation and Maintenance Plans must be prepared by all holders of Permits other than a Basic ACDP. All sources subject to regular permit requirements are subject to operation and maintenance requirements.

(2) The purposes of the operation and maintenance plans are to:

(a) Reduce the number of upsets and breakdowns in particulate control equipment;

(b) Reduce the duration of upsets and downtimes; and

(c) Improve the efficiency of control equipment during normal operations.

(3) The operation and maintenance plans should consider, but not be limited to, the following:

(a) Personnel training in operation and maintenance;

(b) Preventative maintenance procedures, schedule and records;

(c) Logging of the occurrence and duration of all upsets, breakdowns and malfunctions which result in excessive emissions;

(d) Routine follow-up evaluation of upsets to identify the cause of the problem and changes needed to prevent a recurrence;

(e) Periodic source testing of pollution control units as required by the permit;

(f) Inspection of internal wear points of pollution control equipment during scheduled shutdowns; and

(g) Inventory of key spare parts.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468.020 & 468A.025
Hist.: DEQ 6-1983, f. & ef. 4-18-83; DEQ 22-1989, f. & cert. ef. 9-26-89; DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 4-1995, f. & cert. ef. 2-17-95; DEQ 10-1995, f. & cert. ef. 5-1-95; DEQ 22-1996, f. & cert. 10-22-96; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0044; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0210**

**Continuous Monitoring**

(1) The Department will require the installation and operation of instrumentation for measuring and recording emissions and/or the parameters which affect the emission of air contaminants from wood-waste fired boilers, veneer dryers, fiber dryers, and particle dryers to ensure that the sources and the air pollution control equipment are operated at all times at their full efficiency and effectiveness so that the emission of air contaminants is kept at the lowest practicable level. The instrumentation must be periodically calibrated. The method and frequency of calibration must be approved in writing by the Department. Continuous monitoring equipment and operation must be in accordance with continuous emission monitoring systems guidance provided by the Department and must be consistent, where applicable, with the EPA performance specifications and quality assurance procedures outlined in 40 CFR 60, Appendices B and F, and the Quality Assurance Handbook for Air Pollution Measurement Systems, Volume III. The recorded information must be kept for a period of at least one year and must be made available to the Department upon request.

(2) At a minimum, the monitoring required under paragraph (1) of this section must include:

(a) Continuous monitoring and monthly reporting of carbon monoxide concentration and oxygen concentration for any wood-waste fired boiler with a heat input capacity greater than 35 million BTU/hr or for any wood-waste boiler using a wet scrubber as pollution control equipment and steam production rate for any wood-waste fired boiler;

(b) Continuous monitoring and monthly reporting of pressure drop, scrubber water pressure, and scrubber water flow or other parameters deemed by the Department to be equal or better indicators of proper operation of the wet scrubber used as pollution control equipment for any wood-waste fired boiler, veneer dryer, particle dryer, or fiber dryer.

(c) Continuous monitoring and monthly reporting of opacity for any wood-waste fired boiler not controlled by a wet scrubber.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

[Publications: Publications referenced are available from the agency.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468.020 & 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 22-1989, f. & cert. ef. 9-26-89; DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 22-1996, f. & cert. 10-22-96; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0050; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0220**

**Source Testing**

(1) The person responsible for the following sources of particulate emissions must make or have made tests to determine the type, quantity, quality, and duration of emissions, and/or process parameters affecting emissions, in conformance with test methods on file with the Department at the following frequencies:

(a) Wood Waste Boilers with heat input capacity greater than 35 million Btu/hr. -- Once every year;

(b) Veneer Dryers -- Once every year during 1991, 1992, and 1993 and once every 3 years thereafter;

(c) Wood Particle Dryers at Hardboard and Particleboard Plants -- Once every year;

(d) Charcoal Producing Plants -- Once every year.

(e) Wood Waste Boilers with heat input capacity equal to or less than 35 million BTU/hr with dry emission control equipment -- Once in 1992 and once every 3 years thereafter.

(2) Source testing must begin at these frequencies within 90 days of the date by which compliance is to be achieved for each individual emission source.

(3) These source testing requirements will remain in effect unless waived in writing by the Department because of adequate demonstration that the source is consistently operating at lowest practicable levels, or that continuous emission monitoring systems are producing equivalent information.

(4) Source tests on wood waste boilers must not be performed during periods of soot blowing, grate cleaning, or other abnormal operating conditions. The maximum steaming rate for the boiler may not exceed the average steam production rate measured during the source test by more than ten percent (10%).

(5) Source tests must be performed within 90 days of the startup of air pollution control systems.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468.020 & 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 14-1986, f. & ef. 6-20-86; DEQ 22-1988, f. & cert. ef. 9-26-89; DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 22-1996, f. & cert. 10-22-96; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0055; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0230**

**New Sources**

New sources are required to comply with OAR 340-240-0110(1) and 340-240-0120 through 340-240-0250 immediately upon initiation of operation.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 22-1988, f. & cert. ef. 9-26-89; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0065; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0250**

**Open Burning**

No open burning of domestic waste is allowed on any day or at any time when the Department advises fire permit issuing agencies that open burning is not allowed because of adverse meteorological or air quality conditions.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0070; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**La Grande Urban Growth Area**

**340-240-0300**

**Applicability**

OAR 340-240-0300 through 340-240-0360 apply in the La Grande Urban Growth Area.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0200

**340-240-0310**

**Compliance Schedule for Existing Sources**

(1) Except as provided in sections (2) and (3) of this rule, compliance with applicable requirements of OAR 340-240-0300 through 340-240-0360 for a source that is located in the La Grande Urban Growth Area prior to November 15, 1991 must be demonstrated as expeditiously as possible, but in no case later than the following schedule:

(a) No later than May 15, 1992, the owner or operator must submit Design Criteria and a Notice of Intent to Construct for emission-control systems for Department review and approval; and if the Department disapproves the Design Criteria, the owner or operator must revise the Design Criteria to meet the Department's objections and submit the revised Design Criteria to the Department no later than one month after receiving the Department's disapproval;

(b) No later than three months after receiving the Department's approval of the Design Criteria, the owner or operator must submit to the Department a General Arrangement and copies of purchase orders for any emission-control devices;

(c) No later than eight months after receiving the Department's approval of the Design Criteria, the owner or operator must submit to the Department vendor drawings as approved for construction of any emission-control devices and specifications of any other major equipment in the emission-control system in sufficient detail to demonstrate that the requirements of the Design Criteria will be satisfied;

(d) No later than nine months after receiving the Department's approval of the Design Criteria, the owner or operator must begin construction of any emission-control devices;

(e) No later than sixteen months after receiving the Department's approval of Design Criteria, the owner or operator must complete construction in accordance with the Design Criteria;

(f) No later than May 15, 1994, the owner or operator must demonstrate compliance with the applicable contingency requirements.

(2) Section (1) of this rule does not apply if the owner or operator has demonstrated by May 15, 1992 that the source is capable of being operated and is operated in continuous compliance with applicable requirements of OAR 340-240-0300 through 340-240-0360 and the Department has agreed with the demonstration in writing. The Department may grant an extension until November 15, 1992 for a source to demonstrate compliance under this section. The applicable requirements will be incorporated in the Permit issued to the source.

(3) The Department may adjust the schedule specified in subsections (1)(a) through (e) of this rule if necessary to ensure timely compliance with subsection (1)(f) of this rule or if necessary to conform to an existing compliance schedule with an earlier compliance demonstration date.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0205; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**340-240-0320**

**Wood-Waste Boilers**

No person is allowed to cause or permit the emission into the atmosphere from any wood-waste boiler that is located on a plant site where the total heat input capacity from all wood-waste boilers is greater than 35 million Btu/hr:

(1) Any air contaminant for a period or periods aggregating more than three minutes in any one hour which is equal to or greater than ten percent opacity, unless the permittee demonstrates by source test that the source can comply with the emission limit in section (2) of this rule at higher opacity but in no case are emissions equal or exceed 20 percent opacity for more than an aggregate of three minutes in any one hour allowed. Specific opacity limits will be included in the Permit for each affected source.

(2) Particulate matter in excess of 0.05 grains per standard cubic foot, corrected to 12 percent CO2.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0210; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**340-240-0330**

**Wood Particle Dryers at Particleboard Plants**

(1) No person is allowed to cause or permit the total emission of particulate matter from all wood particle dryers at a particleboard plant site to exceed 0.40 pounds per 1,000 square feet of board produced by the plant on a 3/4" basis of finished product equivalent.

(2) No person is allowed to cause or permit the visible emissions from the wood particle dryers at a particleboard plant to exceed ten percent opacity, unless the permittee demonstrates by source test that the particulate matter emission limit in section (1) of this rule can be achieved at higher visible emissions, but in no case are emissions equal or exceed 20 percent opacity allowed. Specific opacity limits will be included in the Permit for each affected source.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0330; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**340-240-0340**

**Hardboard Manufacturing Plants**

No person is allowed to cause or permit the total emissions of particulate matter from all sources within a hardboard plant, other than press/cooling vents, in excess of 0.25 pounds per 1,000 square feet of hardboard produced on a 1/8" basis of finished product equivalent.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0220; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**340-240-0350**

**Air Conveying Systems**

(1) No person is allowed to cause or permit the emission of particulate matter in excess of 0.1 grains per standard cubic foot from any air conveying system emitting less than or equal to ten tons of particulate matter to the atmosphere during any 12-month period beginning on or after January 1, 1990.

(2) All air conveying systems emitting greater than ten tons of particulate matter to the atmosphere during any 12-month period beginning on or after January 1, 1990 must be equipped with a control system with a collection efficiency of at least 98.5 percent or equivalent control as approved by the Department.

(3) No person is allowed to cause or permit the emission of any air contaminant which is equal to or greater than five percent opacity from any air conveying system subject to section (2) of this rule.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0225; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**340-240-0360**

**Fugitive Emissions**

The owner or operator of a large sawmill, any plywood mill or veneer manufacturing plant, particleboard plant, hardboard plant, or charcoal manufacturing plant that is located in the La Grande Urban Growth Area must comply with OAR 340-240-0180.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0230; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**The Lakeview Urban Growth Area**

**340-240-0400**

**Applicability**

OAR 340-240-0400 through 340-240-0440 apply to the Lakeview Urban Growth Area.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 10-1995, f. & cert. ef. 5-1-95; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0300; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**340-240-0410**

**Control of Fugitive Emissions**

(1) Large sawmills, all plywood mills and veneer manufacturing plants, particleboard and hardboard plants, charcoal manufacturing plants, stationary asphalt plants, stationary rock crushers, and sources subject to OAR 340-240-0420 must prepare and implement site-specific plans for the control of fugitive emissions.

(2) Fugitive emission control plans must identify reasonable measures to prevent particulate matter from becoming airborne. Such reasonable measures include, but not be limited to the following:

(a) Scheduled application of asphalt, oil, water, or other suitable chemicals on unpaved roads, log storage or sorting yards, materials stockpiles, and other surfaces which can created airborne dust;

(b) Full or partial enclosure of materials stockpiled in cases where application of oil, water, or chemicals are not sufficient to prevent particulate matter from becoming airborne;

(c) Installation and use of hoods, fans, and fabric filters to enclose and vent the handling of dusty materials;

(d) Adequate containment during sandblasting or other similar operations;

(e) Covering, at all times when in motion, open bodied trucks transporting materials likely to become airborne; and

(f) Procedures for the prompt removal from paved streets of earth or other material which does or may become airborne.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 10-1995, f. & cert. ef. 5-1-95; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0310; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**340-240-0420**

**Requirement for Operation and Maintenance Plans**

(1) Operation and Maintenance Plans must be prepared by all holders of Permits other than a Regulated Source ACDP. All sources subject to regular permit requirements are subject to operation and maintenance requirements.

(2) The purposes of the operation and maintenance plans are to:

(a) Reduce the number of upsets and breakdowns in particulate control equipment;

(b) Reduce the duration of upsets and downtimes; and

(c) Improve the efficiency of control equipment during normal operations.

(3) The operation and maintenance plans should consider, but not be limited to, the following:

(a) Personnel training in operation and maintenance;

(b) Preventative maintenance procedures, schedule and records;

(c) Logging of the occurrence and duration of all upsets, breakdowns and malfunctions which result in excessive emissions;

(d) Routine follow-up evaluation of upsets to identify the cause of the problem and changes needed to prevent a recurrence;

(e) Periodic source testing of pollution control units as required by a permit;

(f) Inspection of internal wear points of pollution control equipment during scheduled shutdowns; and

(g) Inventory of key spare parts.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468.020 & ORS 468A.025
Hist.: DEQ-10-1995, f. & cert. ef. 5-1-95; DEQ 22-1996, f. & cert. 10-22-96; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0320; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**340-240-0430**

**Source Testing**

The person responsible for the following sources of particulate emissions must make or have made tests to determine the type, quantity, quality, and duration of emissions, and/or process parameters affecting emissions, in conformance with test methods on file with the Department at the following frequency: Wood Waste Boilers with total heat input capacity equal to or greater than 35 million Btu/hr. -- Once every three years.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468.020 & ORS 468A.025
Hist.: DEQ-10-1995, f. & cert. ef. 5-1-95; DEQ 22-1996, f. & cert. 10-22-96; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0330; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**340-240-0440**

**Open Burning**

No open burning of domestic waste is allowed to be initiated on any day or at any time when the local air stagnation advisory forecasts adverse meteorological or air quality conditions.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ-10-1995, f. & cert. ef. 5-1-95; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0340; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01

**Klamath Falls Nonattainment Area**

**340-240-0500**

**Applicability**

OAR 340-240-0500 through 340-240-0630 apply in the Klamath Falls Nonattainment Area beginning January 1, 2013.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ xx-2013, f. & cert. ef. xx-xx-xx;

**340-240-0510**

**Opacity Standard**

(1) With the exception of fugitive emissions, no person conducting a commercial or industrial activity may cause or permit the emission of any air contaminant into the atmosphere from any stationary source including fuel or refuse burning equipment, that exhibits equal to or greater than 20% opacity for a period or periods aggregating more than three minutes in any one hour.

 (2) Exceptions to sections (1) of this rule: Where the presence of uncombined water is the only reason for failure of any source to meet the requirement of sections (1) of this rule.

 (3) Opacity is determined in accordance with EPA Method 9 of Appendix A to 40 CFR Part 60 or a continuous opacity monitoring system (COMS) installed and operated in accordance with Performance Specification 1 of Appendix B to 40 CFR Part 60.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468.020 & ORS 468A.025.
Hist.: DEQ xx-2012, f. xx-xx-xx, ef. xx-xx-xx;

**340-240-0520**

**Control of Fugitive Emissions**

(1) All sawmills, plywood mills and veneer manufacturing plants, particleboard and hardboard plants, asphalt plants, rock crushers, animal feed manufacturers, and other major industrial facilities as identified by the Department, must prepare and implement site-specific plans for the control of fugitive emissions. The plan must be submitted to the Department for approval in accordance with paragraph (5) below.

(2) Fugitive emission-control plans must identify reasonable measures to prevent particulate matter from becoming airborne, and avoid the migration of material onto the public road system. Such reasonable measures may include, but are not limited to the following:

(a) Paving all roads and areas on which vehicular traffic occurs at the facility;

(b) Scheduled application of water, or other suitable chemicals on unpaved roads, log storage or sorting yards, materials stockpiles, and other surfaces which can create airborne dust. Dust suppressant material must not adversely affect water quality;

(c) Periodic sweeping or cleaning of paved roads and other areas as necessary to prevent migration of material onto the public road system;

(d) Full or partial enclosure of materials stockpiled in cases where application of oil, water, or chemicals are not sufficient to prevent particulate matter from becoming airborne;

(e) Installation and use of hoods, fans, and fabric filters to enclose and vent the handling of dusty materials;

(f) Adequate containment during sandblasting or other similar operations;

(g) Covering, at all times when in motion, open bodied trucks transporting materials likely to become airborne; and

(h) Procedures for the prompt removal of earth or other material from paved streets.

(3) Reasonable measures may include landscaping and using vegetation to reduce the migration of material onto public and private roadways or from becoming airborne.

(4) The facility owner or operator must supervise and control fugitive emissions and material that may become airborne caused by the activity of outside contractors delivering or removing materials at the site.

(5) For existing sources, the site-specific fugitive emissions control plan must be submitted to the Department by July 1, 2013. For sources that obtain their initial permit after December 14, 2012, the site-specific fugitive emission control plan must be submitted within 60 days after permit issuance. For portable sources that move into the nonattainment area after December 14, 2012, the site-specific fugitive emission control plan must be submitted with the relocation notification. Unless otherwise notified by the Department, the fugitive emission control plan will be approved by default within 30 days after the plan is submitted to the Department. The Department may request revisions to the plan at any time if fugitive emissions are not adequately controlled as demonstrated by visible emissions.

 [**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ xx-xxxx, f. & cert. ef. xx-xx-xx;

**340-240-0530**

**Requirement for Operation and Maintenance Plans**

(1) With the exception of basic and general permit holders, a permit holder must prepare Operation and Maintenance Plans. All sources subject to regular permit requirements are subject to operation and maintenance requirements.

(2) The purposes of the operation and maintenance plans are to:

(a) Reduce the number of upsets and breakdowns in particulate control equipment;

(b) Reduce the duration of upsets and downtimes; and

(c) Improve the efficiency of control equipment during normal operations.

(3) The operation and maintenance plans should consider, but not be limited to, the following:

(a) Personnel training in operation and maintenance;

(b) Preventative maintenance procedures, schedule and records;

(c) Logging of the occurrence and duration of all upsets, breakdowns and malfunctions which result in excessive emissions;

(d) Routine follow-up evaluation of upsets to identify the cause of the problem and changes needed to prevent a recurrence;

(e) Periodic source testing of pollution control units as required by the permit;

(f) Inspection of internal wear points of pollution control equipment during scheduled shutdowns; and

(g) Inventory of key spare parts.

(4) Existing sources must submit an Operation and Maintenance Plan to the Department by July 1, 2013. Sources obtaining an initial permit after December 14, 2012 must submit the Operation and Maintenance within 60 days of permit issuance. The Department will notify sources within 30 days of plan submittal only if the Operation and Maintenance Plan is not approved. The Department may request revisions to the plan at any time if plans are not sufficient.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468.020 & 468A.025
Hist.: DEQ xx-xxxx, f. & ef. xx-xx-xx;

**340-240-0540**

**Compliance Schedule for Existing Industrial Sources**

(1) Except as provided in sections (2) and (3) of this rule, compliance with applicable requirements of OAR 340-240-0500 through 340-240-0540 for a source that is built and located in the Klamath Falls Nonattainment Area prior to December 14, 2012 must be demonstrated by the owner or operator of the source as expeditiously as possible, but in no case later than the following schedule:

(a) No later than June 15, 2013, the owner or operator must submit Design Criteria and a Notice of Intent to Construct for emission-control systems for complying with OAR 340-240-0510 through 340-240-0540 for Department review and approval; If the Department disapproves the Design Criteria, the owner or operator must revise the Design Criteria to meet the Department's objections and submit the revised Design Criteria to the Department no later than one month after receiving the Department's disapproval;

(b) No later than three months after receiving the Department's approval of the Design Criteria, the owner or operator must submit to the Department copies of purchase orders for any emission-control devices;

(c) No later than eight months after receiving the Department's approval of the Design Criteria, the owner or operator must submit to the Department vendor drawings as approved for construction of any emission-control devices and specifications of any other major equipment in the emission-control system in sufficient detail to demonstrate that the requirements of the Design Criteria will be satisfied;

(d) No later than nine months after receiving the Department's approval of the Design Criteria, the owner or operator must begin construction of any emission-control devices;

(e) No later than sixteen months after receiving the Department's approval of Design Criteria, the owner or operator must complete construction in accordance with the Design Criteria;

(f) No later than October 15, 2014, the owner or operator must demonstrate compliance with the applicable requirements identified in OAR 340-240-500 through 340-240-540.

(2) Section (1) of this rule does not apply if the owner or operator of the source has demonstrated by September 15, 2014 that the source is capable of being operated and is operated in continuous compliance with applicable requirements of OAR 340-240-0500 through 340-240-0540 and the Department has agreed with the demonstration in writing. The Department may grant an extension until April 15, 2015 for a source to demonstrate compliance under this section. The applicable requirements will be incorporated in the Permit issued to the source.

(3) The Department may adjust the schedule specified in subsections (1)(a) through (e) of this rule if necessary to ensure timely compliance with subsection (1)(f) of this rule or if necessary to conform to an existing compliance schedule with an earlier compliance demonstration date.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ xx-2012, f. & cert. ef. xx-xx-xx;

**340-240-0550**

**Requirements for New Sources When Using Residential Wood Fuel-Fired Device Offsets**

(1) All new or modified sources subject to OAR 340-224-0050 or 340-224-0060 may opt to use wood fuel-fired device emission reductions from within the nonattainment or maintenance area to satisfy the offset requirements of OAR 340-225-0090(2):

(a) Offsets for decommissioning fireplaces and non-certified woodstoves (including fireplace inserts) are obtained at a ratio of at least 1:1 (i.e., one ton of emission reductions from fireplaces and non-certified wood stoves offsets one ton of emissions from a proposed new or modified industrial point source proposed to be located inside or impacting the non-attainment area) or maintenance area;

(b) Offsets must be obtained from within the Klamath Falls Nonattainment Area; and

(c) The emission reductions offsets must be approved by the Department and comply with OAR 340-240-0560.

(2) The net air quality benefit analysis specified in OAR 340-225-0090(2)(a)(E) is not applicable to offsets meeting the criteria in (a) through (c) of section (1) of this rule.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468.020 & 468A.025
Hist.: DEQ xx-xxxx, f. & ef. xx-xx-xx;

**Real and Permanent PM2.5 and PM10 Offsets**

**340-240-0560**

(1) Annual emissions reductions offsets (PM2.5 and PM10) are determined as follows:

(a) For **fireplaces**, the emission reductions offsets for decommissioning the fireplace and replacing it with a:

(A) certified fireplace insert is 0.02 tons for each replaced device;

(B) pellet stove insert is 0.03 tons for each replaced device; or

(C) alternative non-wood burning heating system is 0.04 tons for each replaced device.

**Note:** As used in this rule, “Certified” includes catalytic and non-catalytic designs, unless otherwise specified.

(b) For **non-certified fireplace inserts**, the emission reduction for replacing the heating device with a:

(A) certified fireplace insert is 0.02 tons for each replaced device;

(B) pellet stove is 0.04 tons for each replaced device; or

(C) alternative non-wood burning heating system is 0.04 tons for each replaced device

(c) For **conventional (non-certified) woodstoves**, the emission reduction for replacing the heating device with a:

(A) certified woodstove or certified fireplace insert is 0.03 tons for each replaced device; or

(B) pellet stove is 0.05 tons for each replaced device; or

(C) alternative non-wood burning heating system is 0.06 tons for each replaced device

(d) For **certified woodstoves**, the emission reduction for replacing the heating device with a:

(A) pellet stove is 0.03 tons for each replaced device; or

(B) alternative non-wood burning heating system is 0.04 tons for each replaced device

(2) For the emission reductions identified in section (1) to be considered permanent, the person responsible for taking credit for the emission reductions must obtain and maintain the following records for at least 5 years from the date that the proposed industrial point source commences operation:

(a) the address of the residence where the emission reduction occurred;

(b) the date that the emission reduction was achieved;

(c) purchase and installation records for certified woodstoves, certified inserts, or alternative non-wood burning heating systems;

(d) records for permanently decommissioning fireplaces, if applicable; and

(f) disposal records for non-certified woodstoves or fireplace inserts removed.

(3) The records identified in section (2) may be provided by a third party authorized and monitored by the DEQ to procure the emission reductions identified in section (1).

(4) All emission reductions must be achieved prior to startup of the proposed source using the emission reductions as offsets in the permitting action specified in OAR 340-224-0050 or 340-224-0060.

**Klamath Falls Nonattainment Area Contingency Measures**

**340-240-0570**

**Applicability**

OAR 340-240-0570 through 340-240-0630 apply to the Klamath Falls Nonattainment Area for PM2.5 should the area not achieve attainment by the applicable Clean Air Act deadline.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.480
Hist.: DEQ xx-xxxx, f. & cert. ef. xx-xx-xx;

**340-240-0580**

**Existing Industrial Sources Control Efficiency**

The owner or operator of an Oregon Title V Operating Permit program source, as defined in OAR 340-200-0020 may not remove or modify existing control devices unless the new control device has the same or better PM2.5 control efficiency as the old device.

**340-240-0590**

**Particulate Emission Limitations for Industrial Sources**

 (1) No person may cause, suffer, allow, or permit particulate matter emissions from any wood-fired boiler in excess of: 0.1 grains per standard cubic foot, corrected to 12 percent CO2. Particulate matter emissions are measured in accordance with Oregon DEQ Method 5.

(2) No person may cause, suffer, allow, or permit particulate matter emissions from any air contaminant source other than boilers and fugitive emission sources in excess of: 0.1 grains per standard cubic foot. Particulate matter emissions are measured in accordance with Oregon Methods 5, 7, or 8, as specified by DEQ in an approved source test plan.

 [**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468.020 & ORS 468A.025.
Hist.: DEQ xx-2012, f. xx-xx-xx, ef. xx-xx-xx;

**340-240-600**

**Contingency Measures: Schedule for Compliance** **for Existing Industrial Sources**

Additional control equipment required to meet contingency requirements described in OAR 340-240-0590 must be implemented on a compliance schedule.

(1) Except as provided in sections (2) and (3) of this rule, the owner or operator of a source located in the Klamath Falls Nonattainment Area prior to December 14, 2014, must demonstrate compliance with the applicable requirements of OAR 340-240-0570 through 340-240-0590 as expeditiously as possible, but in no case later than the following schedule:

(a) No later than June 15, 2015, the owner or operator must submit Design Criteria and a Notice of Intent to Construct for emission-control systems for Department review and approval. If the Department disapproves the Design Criteria, the owner or operator must revise the Design Criteria to meet the Department's objections and submit the revised Design Criteria to the Department no later than one month after receiving the Department's disapproval;

(b) No later than three months after receiving the Department's approval of the Design Criteria, the owner or operator must submit to the Department copies of purchase orders for any emission-control devices;

(c) No later than eight months after receiving the Department's approval of the Design Criteria, the owner or operator must submit to the Department vendor drawings for construction of any emission-control devices and any other major equipment in the emission-control system in sufficient detail to demonstrate that the requirements of the Design Criteria will be satisfied;

(d) No later than nine months after receiving the Department's approval of the Design Criteria, the owner or operator must begin construction of any emission-control devices;

(e) No later than sixteen months after receiving the Department's approval of Design Criteria, the owner or operator must complete construction in accordance with the Design Criteria;

(f) No later than December 15, 2016, the owner or operator must demonstrate compliance by conducting a source test with the applicable contingency requirements.

(2) Section (1) of this rule does not apply if the owner or operator has demonstrated by September 15, 2015 that the source is capable of being operated and is operated in continuous compliance with applicable requirements of OAR 340-240-0570 through 340-240-0590 and the Department has agreed with the demonstration in writing. The Department may grant an extension until April 15, 2017 for a source to demonstrate compliance under this section. The applicable requirements will be incorporated in the Permit issued to the source.

(3) The Department may adjust the schedule specified in subsections (1)(a) through (e) of this rule if, necessary, to ensure timely compliance with subsection (1)(f) of this rule or if necessary to conform to an existing compliance schedule with an earlier compliance demonstration date.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & ORS 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ xx-2012, f. & cert. ef. xx-xx-xx;

**340-240-0610**

**Continuous Monitoring for Industrial Sources**

(1) The owner or operator of an Oregon Title V Operating Permit program source, as defined in OAR 340-200-0020 must install and operate instrumentation for measuring and recording emissions or the parameters that affect the emission of air contaminants from wood-fired boilers, veneer dryers, fiber dryers, and particle dryers to ensure that the sources and the air pollution control equipment are operated at all times at their full efficiency and effectiveness so that the emission of air contaminants is kept at the lowest practicable level. Continuous monitoring equipment and operation must be in accordance with the Department’s Continuous Monitoring Manual.

(2) At a minimum, the monitoring required under paragraph (1) of this section must include:

 (a) Continuous monitoring of control device parameters for any wood- fired boiler, veneer dryer, particle dryer, or fiber dryer.

(b) Continuous monitoring of opacity for any wood- fired boiler not controlled by a wet scrubber.

[**NOTE:** This rule is included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

[Publications: Publications referenced are available from the agency.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468.020 & 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 22-1989, f. & cert. ef. 9-26-89; DEQ 23-1991, f. & cert. ef. 11-13-91; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 22-1996, f. & cert. 10-22-96; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0050; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0620**

**Contingency Measures: New Industrial Sources**

New industrial sources must comply with OAR 340-240-0570 through 340-240-0610 immediately upon receiving an Air Contaminant Discharge Permit or an Oregon Title V Operating Permit.

[**NOTE:** These rules are included in the State of Oregon Clean Air Act Implementation Plan as adopted by the Environmental Quality Commission under OAR 340-200-0040.]

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468A.025
Hist.: DEQ 4-1978, f. & ef. 4-7-78; DEQ 22-1988, f. & cert. ef. 9-26-89; DEQ 4-1993, f. & cert. ef. 3-10-93; DEQ 14-1999, f. & cert. ef. 10-14-99, Renumbered from 340-030-0065; DEQ 6-2001, f. 6-18-01, cert. ef. 7-1-01; DEQ 1-2005, f. & cert. ef. 1-4-05

**340-240-0630**

**Contingency Enhanced Curtailment of Use of Solid Fuel Burning Devices and Fireplaces**

1. No fireplace, as defined by OAR 340-362-0450, installed after March 1, 2015, may emit more than 5.1 grams per kilogram of particulate emissions.  A new fireplace shall be deemed in compliance with this emission standard if, when installed, it has been certified either in accordance with ASTM international standard test method E2558 or by the Department pursuant to OAR 340-262-0500.  A fireplace installed after March 1, 2015, that is not certified as described in this rule shall be presumed not to comply with this rule.

Stat. Auth.: ORS 468 & 468A
Stats. Implemented: ORS 468A.010 to 468A.025
Hist.: DEQ xx-xxx, f. & ef. xx-xx-xx;