|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| OAR 340-202-0210PSD Increments (Maximum Allowable Increase) Micrograms per cubic meter |
| **CLASS I** |
| *Pollutant* | *Micrograms per cubic meter*  |
| Particulate matter:PM10, Annual arithmetic mean PM10, 24-hour maximum | 48 |
| Sulfur dioxide:Annual arithmetic mean24-hour maximum 3-hour maximum  | 25 25  |
| Nitrogen dioxide:Annual arithmetic mean  |  2.5 |
| **Class II** |
| *Pollutant* | *Micrograms per cubic meter* |
| Particulate matter: PM10, Annual arithmetic mean PM10, 24-hour maximum | 1730 |
| Sulfur dioxide: Annual arithmetic mean24-hour maximum 3-hour maximum  | 20 91512  |
| Nitrogen dioxide: Annual arithmetic mean  | 25  |
| **Class III** |
| *Pollutant* | *Micrograms per cubic meter* |
| Particulate matter: PM10, Annual arithmetic mean PM10, 24-hour maximum | 3460  |
| Sulfur dioxide: Annual arithmetic mean24-hour maximum 3-hour maximum  | 40182700  |
| Nitrogen dioxide: Annual arithmetic mean  | 50 |

 |
|  |