|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  | | --- | --- | | OAR 340-202-0210 PSD Increments (Maximum Allowable Increase)  Micrograms per cubic meter | | | **CLASS I** | | | *Pollutant* | *Micrograms per cubic meter* | | Particulate matter:  PM10, Annual arithmetic mean   PM10, 24-hour maximum | 4  8 | | Sulfur dioxide:  Annual arithmetic mean  24-hour maximum   3-hour maximum | 2  5  25 | | Nitrogen dioxide:  Annual arithmetic mean | 2.5 | | **Class II** | | | *Pollutant* | *Micrograms per cubic meter* | | Particulate matter:  PM10, Annual arithmetic mean   PM10, 24-hour maximum | 17  30 | | Sulfur dioxide:  Annual arithmetic mean  24-hour maximum   3-hour maximum | 20  91  512 | | Nitrogen dioxide:  Annual arithmetic mean | 25 | | **Class III** | | | *Pollutant* | *Micrograms per cubic meter* | | Particulate matter:  PM10, Annual arithmetic mean   PM10, 24-hour maximum | 34  60 | | Sulfur dioxide:  Annual arithmetic mean  24-hour maximum   3-hour maximum | 40  182  700 | | Nitrogen dioxide:  Annual arithmetic mean | 50 | |
|  |