|  |
| --- |
| C:\Users\mgoldst\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.Word\LogoColorRegular.png**OAR 340-035-0030****Table 2****In-Use Road Vehicle Standards****Stationary Test** |
| **Model Year** | **Maximum Noise Level (dBA)** | **Minimum Distance from Vehicle to Measurement Point** |
| **All Vehicles Described in ORS 481.205(2)** |
| Before 1976 | 94 | 25 feet (7.6 meters) |
| 1976 and after | 91 | 25 feet (7.6 meters) |
| **All Other Trucks in Excess of 8,000 pounds (3629 kg.) GVRW** |
| Before 1976 | 94 | 25 feet (7.6 meters) |
| 1976-1981 | 91 | 25 feet (7.6 meters) |
| After 1981 | 88 | 25 feet (7.6 meters) |
| **Motorcycles** |
| 1975 and Before | 102 | 20 inches (1/2 meter) |
| After 1975 | 99 | 20 inches (1/2 meter) |
| **Front-engine Automobiles, Light Trucks, All Other Front-engine Road Vehicles** |
| All | 95 | 20 inches (1/2 meter) |
| **Rear-engine Automobiles, Light Trucks and All Other Front-engine Road Vehicles** |
| All | 95 | 20 inches (1/2 meter) |
| **Buses as Defined Under ORS 481.030** |
| Before 1976 | 94 | 25 feet (7.6 meters) |
| 1976 and After | 91 | 25 feet (7.6 meters) |