**CHLORINE ROOM INJECTION VALVES**

**THIS THREADED FITTING REQUIRES THREAD PASTE AND NO MORE THAN 1-1½ TURNS PAST HAND TIGHT. IF LEAKING REMOVE AND REAPPLY THREAD PASTE/SEALANT. THREADED FITTINGS CRACK EASILY.**

**THESE 2 FITTINGS ARE “HAND” TIGHT ONLY AND NO THREAD SEALANT.**

**PUSH DISARM RE-ARM BUTTON TO CLEAR ALARMS**

