**Imbedded General Permit**

**1 MGD**

**1 ug/l**

**Sludge**

**Mass out**

**Process**

**0.2 MGD**

**Non-Process**

**0.8 MGD**

**0.2 MGD**

**1 ug/l**

**0.2 MGD**

**EL = < 5 ug/l**

RPA here for Individual permit

* Intake Credit & WQBEL?

Types of General Permit Conditions: e.g.

* <5X increase in concentration (Avg.)
* > 30:1 dilution
* < 0.5, 1, 0.2 MGD depending on process type (single pass, multi-pass, electric, etc.)
* Sludge to SW, no backwash

**General Permit**

**0.2 MGD**

**EL = < 5 ug/l**

General Permit here w/deminimus

**Non-Process**

**1 MGD**

**1 ug/l**

**Sludge**

**Mass out**