|  |  |
| --- | --- |
| **TABLE 2**  **OAR 340-200-0020**  **SIGNIFICANT EMISSION RATES** | |
| ***Pollutant*** | ***Emission Rate*** |
| Greenhouse Gases (CO2e) | 75,000 tons/year |
| Carbon Monoxide | 100 tons/year |
| Nitrogen Oxides (NOX) | 40 tons/year |
| Particulate Matter | 25 tons/year |
| PM10 | 15 tons/year |
| Direct PM2.5 | 10 tons/year |
| PM2.5 precursors (SO2 or NOx) | 40 tons/year |
| Sulfur Dioxide (SO2) | 40 tons/year |
| Volatile Organic Compounds (VOC) | 40 tons/year |
| Ozone precursors (VOC or NOx) | 40 tons/year |
| Lead | 0.6 ton/year |
| Fluorides | 3 tons/year |
| Sulfuric Acid Mist | 7 tons/year |
| Hydrogen Sulfide | 10 tons/year |
| Total Reduced Sulfur (including hydrogen sulfide) | 10 tons/year |
| Reduced sulfur compounds (including hydrogen sulfide) | 10 tons/year |
| Municipal waste combustor organics (measured as total tetra- through octa- chlorinated dibenzo-p-dioxins and dibenzofurans) | 0.0000035 ton/year |
| Municipal waste combustor metals (measured as particulate matter) | 15 tons/year |
| Municipal waste combustor acid gases (measured as sulfur dioxide and hydrogen chloride) | 40 tons/year |
| Municipal solid waste landfill emissions (measured as nonmethane organic compounds) | 50 tons/year |