|  |
| --- |
| **pansm.tiffState of Oregon Department of Environmental Quality**  **Significant Air Quality Impact**  **Table 1 – OAR 340-200-0020** |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | Pollutant | Averaging Time | Air Quality Area Designation | | | | Class I | Class II | Class III | | SO2 (µg/m3)\* | Annual | 0.10 | 1.0 | 1.0 | | 24-hour | 0.20 | 5.0 | 5.0 | | 3-hour | 1.0 | 25.0 | 25.0 | | 1-hour | --- | 8 | --- | | PM10 (µg/m3) | Annual | 0.20 | 0.2 | 0.2 | | 24-hour | 0.30 | 1.0 | 1.0 | | PM2.5 (µg/m3) | Annual | 0.06 | 0.3 | 0.3 | | 24-hour | 0.07 | 1.2 | 1.2 | | NO2 (µg/m3) | Annual | 0.10 | 1.0 | 1.0 | | 1-hour | --- | 8 | --- | | CO (mg/m3)\*\* | 8 hour | --- | 0.5 | 0.5 | | 1-hour | --- | 2.0 | 2.0 | | \* micrograms/cubic meter  \*\*milligrams/cubic meter | | | | | |

|  |  |
| --- | --- |
|  |  |