|  |
| --- |
| **pansm.tiffState of Oregon Department of Environmental Quality** **Significant Air Quality Impact** **Table 1 – OAR 340-200-0020** |
|

|  |  |  |
| --- | --- | --- |
| Pollutant | Averaging Time | Air Quality Area Designation |
| Class I | Class II | Class III |
| SO2 (µg/m3)\* | Annual | 0.10 | 1.0 | 1.0 |
| 24-hour | 0.20 | 5.0 | 5.0 |
| 3-hour | 1.0 | 25.0 | 25.0 |
| 1-hour | --- | 8 | --- |
| PM10 (µg/m3) | Annual | 0.20 | 0.2 | 0.2 |
| 24-hour | 0.30 | 1.0 | 1.0 |
| PM2.5 (µg/m3) | Annual | 0.06 | 0.3 | 0.3 |
| 24-hour | 0.07 | 1.2 | 1.2 |
| NO2 (µg/m3) | Annual | 0.10 | 1.0 | 1.0 |
| 1-hour | --- | 8 | --- |
| CO (mg/m3)\*\* | 8 hour | --- | 0.5 | 0.5 |
| 1-hour | --- | 2.0 | 2.0 |
| \* micrograms/cubic meter\*\*milligrams/cubic meter |

 |

|  |  |
| --- | --- |
|  |  |