**OAR 340-220-0150 - Equation**

**Determining VOC Emissions Using Material Balance**

**VOCtot = VOCadd - VOCcons**

Where:

* VOCtot = Total VOC emissions, tons
* VOCadd = VOC added to the process, tons
* VOCcons = VOC consumed and/or recovered from the process, tons