|  |  |  |  |
| --- | --- | --- | --- |
| C:\Users\mgoldst\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.Word\LogoColorRegular.png**OAR 340-035-0030**  **Table 3**  **In-Use Road Vehicle Standards**  **Moving Test at 50 feet (15.2 meters) or Greater at Vehicle Speed** | | | |
| **Operating Conditions** | **Trucks and Buses Exceeding 10,000 pounds GVWR** | **Automobiles and Light Trucks** | **Motorcycles** |
| **Posted 45 mph or less Under any Grade, Load, Acceleration or Deceleration** | 86 | 72 | 78 |
| **Posted Greater Than 45 mpg Under any Grade, Load, Acceleration or Deceleration** | 90 | 78 | 62 |
| **Moving at 35 mph or Less on Level Roadway Under Constant Speed More than 200 Feet From Stop** | 84 | 70 | 74 |