April 5, 2026 
DEQ Comments for 6565 Baxter and Flaming 2026-04-17 Soil Vapor Sampling Work Plan

On behalf of Truck Terminals Inc, AEI Consultants (AEI) has prepared this Soil Vapor Sampling Work Plan for proposed soil vapor sampling activities at 3717 NW Saint Helens, Portland, Oregon (“the Site”). This work plan has been prepared in response to a request for submittal of a work plan for soil vapor sampling from the Oregon Department of Environmental Quality (DEQ) in a letter dated January 12, 2026.

The catch basins and trench drain were reportedly abandoned (capped) in 1995. The installation date of the catch basins is not known, and it is unknown if they were connected to the septic system or municipal sewer. These features can act as preferential pathways for contaminants such as oil, grease, fuel, or cleaning solvents discharged or released during the former activities to reach and migrate through the subsurface 


